SPEC UPDATE (GCP)

# **Issue:**

SUMMARY: SUMMARY: Token shows SPEC to be NONTLS in ACMS when it should be SVCMUX. Will need to engage GCP to push the change to ACMS per what it shows in ASOC.

# **Sample Ticket:**

Ticket #: **000000225327356**

**Resolution Steps:**

1. Ask user to provide token ID if not provided on the ticket.
2. Check SPEC in ASOC for that token.

select spec from Ethernet\_token where token\_id = 'ETH5929658';

1. Create ticket to GCP to update speccode in GCP.
2. Provide this query on ticket.

update acms.accessqualification set SPECCODE = 'SVCMUX' where tokenid = 'ETH5929658';